Village of Payne CSO Annual Report

(May 1, 2019 – May 1, 2020)

* CSO Locations:
1. 002 - State Route 500 Inlet 40” Overflow 40” with 2 swing checks
2. 003 – Fox Street Inlet 10” overflow 8”
* No CSO discharge for the calendar year noted
* No Public access areas affected
* Permitte Contact information can also be found at Payne village hall located at (119 N. Main St. Payne, OH 45880 Phone: 419-263-2514
* The Village has put in and maintained a retention pond located at (Fox Street Off State Route 500) Which the Village and EPA hopes to limit overflows to one or less a year depend on precipitation
* If any discharge is seeing please contact Allen Wobler, Payne City Supervisor, 419-263-8090 Email: Waterdept@villageofpayne.com , Or John Hall, BPA President, 419-399-7530 Email: bjhall42@yahoo.com
* Minimum control:
	+ The village provides proper operation and maintenance for the cso and sewer system
	+ The village uses the storage system during wet weather to its maximum capacity before allowing an overflow
	+ The village reviews and modifies local programs to minimize t impact f nondomestic discharges from combined sewer overflows
	+ The village maximizes the capabilities of the POTW to treat we weather flows and maximize wet weather flow to wastewater plant within the limits of the plant
	+ The village prohibit dry weather overflows
	+ The village controls solid floatable materials in combined sewer overflow
	+ The village does the required inspection, monitoring and reporting of CSO
	+ The village does pollution prevention programs that focus on reducing the level of contaminants in cso
	+ The village implements a public notification programs of areas affected by CSO through a website and posted signs